{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["明细"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"明细","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
["海口医院综合布线材料清单"]
["序号","产品（项目）名称","规格","描述","单位","数量"]
[1,"六类信息模块",null,"白色，RJ45，镀金50μ\"","个",64]
[2,"面板(语音/数据标识条)",null,"白色，可装2个模块","个",64]
[3,"六类24口数据配线架(带24个模块)",null,"高度1U，黑色","个",3]
[4,"六类非屏蔽线缆",null,"UTP型，灰色，305米/箱","箱",16]
[5,"六类跳线",null,"RJ45,灰色(2m)","条",64]
[6,"六类跳线",null,"RJ45,灰色(3m)","条",64]
[7,"12芯室外单模光纤","12芯","室外单模12芯圆形配线光缆(单模, 9/125)","米",300]
[8,"ODF架","36口","36口机柜式光纤配线架高度1U","个",4]
[9,"ODF架","12口","12口机柜式光纤配线架高度1U","个",3]
[10,"单模模FC光纤耦合器","FC","陶瓷插芯,单模","个",72]
[11,"单模模光纤尾纤（5FT）","FC-FC","FC-FC(3米) 单模跳线","条",72]
[12,"光纤熔接",null,"FC","芯",72]
[13,"布线机柜","600*600*2000","外观高贵典雅，工艺精湛、尺寸精密，媲美国际最高档网络服务器机柜，彰显优质机房工程形象；可方便地安装图腾机柜集中配电单元（专利）  容量 42U 尺寸 0.6(宽)×0.6(深)×1.999(高) 颜色 黑色 标准 符合ANSI/EIA RS-310-D, IEC297-2, DIN41491; PART1, DIN41494; PART7, GB/T3047.2- 92标准; 兼容ETSI标准 门/门锁 高通风率六角弧形网孔前门(专利), 双开六角网孔后门及三段侧门; 月光旋把机柜门锁 材料/工艺 SPCC优质冷扎钢板制作; 厚度:方孔条2.0mm, 托盘2.0mm, 安装梁1.5m, 其他1.2mm; 表面处理:脱脂、酸洗、磷化、静电喷塑 功能描述 外观高贵典雅, 工艺精湛、尺寸精密","个",3]
[14,"PDU","8孔10A","8孔10A","个",3]
[15,"底盒（PVC）","86型","86型","个",64]
[16,"理线架",null,"高度1U，黑色","个",3]
[17,"PVC管","20/25","20或25及其配件","米",640]