{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["网络设备清单"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"网络设备清单","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["无线、汇聚、安全网络设备清单"]
["序号","设备名称","品牌","规格型号","单位","数量","备注"]
["一","第一期无线系统"]
[1,"移动医护无线网络综合网关","锐捷","RG-WS7216-S","台",1]
[2,"移动医护终端接入认证系统","锐捷","RG-M7000-WS","台",1]
[3,"移动医护业务无线AP","锐捷","RG-AP4220","台",50]
[4,"移动医护业务无线信号分配AP","锐捷","RG-APD-M(EA)","台",233]
[5,"无菌空间无线覆盖AP","锐捷","RG-AP130(W2)","台",29]
[6,"移动医护无线系统连接线缆A类","锐捷","RG-DCAB-SMA-5m","根",122]
[7,"移动医护无线系统连接线缆B类","锐捷","RG-DCAB-SMA-10m","根",1398]
[8,"移动医护无线系统连接线缆C类","锐捷","RG-Cab-SMA-18m-MJ","根",50]
[9,"移动医护无线系统连接线缆D类","锐捷","RG-Cab-SMA-35m-MJ","根",180]
[10,"移动医护无线系统无线AP天线","锐捷","RG-IOA-2503-X5","台",1520]
[11,"POE交换机","锐捷","RG-S2910-24GT4SFP-UP-H(V3.0)","台",45]
["二","第一期无线系统增补"]
[1,"AC授权","锐捷","RG-LIC-WS-32","项",1]
[2,"移动医护业务无线AP","锐捷","RG-AP4220","台",2]
[3,"移动医护业务无线信号分配AP","锐捷","RG-APD-M(EA)","台",6]
[4,"移动医护无线系统连接线缆B类","锐捷","RG-DCAB-SMA-10m","根",24]
[5,"移动医护无线系统连接线缆D类","锐捷","RG-Cab-SMA-35m-MJ","根",6]
[6,"移动医护无线系统无线AP天线","锐捷","RG-IOA-2503-X5","台",24]
[7,"POE交换机","锐捷","RG-S2910-24GT4SFP-UP-H(V3.0)","台",1]
[]
["三","机房汇聚网络设备"]
[1,"核心路由器","华为","AR0M0024BA00\nAR0MWMF9TT00","套",1]
[2,"核心路由器","华为","AR2240C\nAR01SRU2C","套",1]
[3,"汇聚交换机","华为","S7706及板卡模块","套",1]
[4,"汇聚交换机","华为","5700光电口及电口","台",5]
["四","防火墙安全设备"]
[1,"SSL VLN","深信服","VPN-1000","套",1]
[2,"防火墙","深信服","AF-1880","套",1]
[3,"防火墙","深信服","AF-1880","套",1]
[4,"防火墙","深信服","AF-1880","套",1]